Author: Channing Applegarth

Save MONEY with ElectroLIFE

ElectroLIFE offers GREEN CLEANING TECHNOLOGY:
ELIMINATES all detergents, microbes, metals, and any other toxic and non-toxic additives from brewery tailing water
PROVIDES both acidic and alkaline water for cleaning without the need for additional chemicals or cleaners using just our technology, water and electricity
MITIGATES your risk of dirty water incidents with the EPA and ELIMINATES associated fines
REMOVES your dependency on expensive additives or chemicals
Ask us how!

Our Mission Statement is simple: Provide a well-designed system and process that an end user can acquire, implement and monitor. ElectroLIFE is simple to operate, easy to maintain, cost effective and reliable. These attributes produce efficiency, energy cost savings and a consistent performance.

Vogel & Brown
Contact: Channing Applegarth
Mobile: 813-846-3568
Email: capplegarth@vogelandbrown.com

The FIRST,
BEST, and ONLY completely GREEN solution for CHEMICAL FREE scale and rust removal!

Customer Illustrations

Throughout Brewing Process

Specifications

High pH Water - 11.5 pH water removes all yeast in the process without additional chemicals
Low pH Water - 2.5* pH water removes all microbes (~300 strains of bacteria & viruses) in the process without additional chemicals
Molecularly altered water is more soluble for a given process since water efficiency increases

Three primary stages can benefit from ElectroLIFE :
As electrolysis occurs in the ElectroLIFE, the molecular structure of the water is changed and aligned which provides greater efficiencies when cooling the water—needs less energy to achieve
During the Mash, ElectroLIFE can stabilize the pH to a specific level at any level between 2.5 - 11.5.
The ElectroLIFE unit can filter impurities and remove waste solids which are flushed from the ElectroLIFE unit. Waste water is clean!

ElectroLIFE throughout the process

DIMENSIONS:	D=350mm (14”), W=700mm (28”), H=1170mm (47”)
WEIGHT:	40 kg (88lbs)
WATER PRESSURE:	Below 0.04 Mpa (0.4 Kg f/cm2)~ 0.2 Mpa (2.0 kgf/cm2) / The pressure resistance of the electrolysis vessel of 0.2 Mpa (2.0 kgf/cm2)
INPUT POWER SOURCE:	Single phase AC 100V~240V, 50/60Hz
MAX. POWER / CONSUMPTION:	800W (Main Frame Maximum of 600W)
WATER TREATMENT / METHOD:	Electrolysis. (Maximum of 10A, Preset Arbitrary Electrical Current) Once scaling is removed 10A is reduced to 5 A.
MAXIMUM FLOW:	25 liters (6.6 gallons) per minute
ELECTROLYSIS VESSEL / SYSTEM:	Continuous flow
LIFE DURATION OF ELECTRODE:	Approximately 2 years
PIPE RADIUS:	Water supply = 1/2B Hose Nipple, Flush & Drainage = 3/4B Hose Nipple