Author: Channing Applegarth

Save MONEY with ElectroLIFE

ElectroLIFE saves you money:
REMOVES harmful scaling and rust in your existing HVAC cooling system using just our technology, water and electricity
PREVENTS scaling and rust from occurring in new and old HVAC systems
REDUCES your total electric consumption, EXTENDING the life of your HVAC system and OPTIMIZING your cooling efficiency
ELIMINATES your dependency on expensive additives or chemicals
Ask us how!

Our Mission Statement is simple: Provide a well-designed system and process that an end user can acquire, implement and monitor. ElectroLIFE is simple to operate, easy to maintain, cost effective and reliable. These attributes produce efficiency, energy cost savings and a consistent performance.

9505 Berger Road
Columbia, MD 21046

Pino DiLullo
After Market Leader
Mobile: 301-520-2403
Email: pinodilullo@havtech.com

The FIRST,
BEST, and ONLY completely GREEN solution for CHEMICAL FREE scale and rust removal!

Customer Illustrations

Process Elements

Specifications

ElectroLife cleaned older HVAC systems in just 2 months:

Below shows how scaling is eliminated due to properties of the circulatory water having taken on a higher level of ionic product and creating heightened dissociation:

10 Years of chemical usage

60 Days of ElectroLIFE

From this to this in 60 days after using ElectroLIFE

Five primary elements of the ElectroLIFE process:
Circulatory water of the HVAC tower passes through it’s reservoir
System Pump transfers the circulatory water from the reservoir through the ElectroLIFE unit
ElectroLIFE unit electrolyzes and filters solids from water
Treated water returns to the reservoir
Waste solids are flushed from ElectroLIFE unit

Schematic

DIMENSIONS:	D=350mm (14”), W=700mm (28”), H=1170mm (47”)
WEIGHT:	40 kg (88lbs)
WATER PRESSURE:	Below 0.04 Mpa (0.4 Kg f/cm2)~ 0.2 Mpa (2.0 kgf/cm2) / The pressure resistance of the electrolysis vessel of 0.2 Mpa (2.0 kgf/cm2)
INPUT POWER SOURCE:	Single phase AC 100V~240V, 50/60Hz
MAX. POWER / CONSUMPTION:	800W (Main Frame Maximum of 600W)
WATER TREATMENT / METHOD:	Electrolysis. (Maximum of 10A, Preset Arbitrary Electrical Current) Once scaling is removed 10A is reduced to 5 A.
MAXIMUM FLOW:	25 liters (6.6 gallons) per minute
ELECTROLYSIS VESSEL / SYSTEM:	Continuous flow
LIFE DURATION OF ELECTRODE:	Approximately 2 years
PIPE RADIUS:	Water supply = 1/2B Hose Nipple, Flush & Drainage = 3/4B Hose Nipple